**FRESCOLORI Croco**

Delivery and servicing surfaces exclusively by trained FRESCOLORI processing specialists, with a long-term guarantee of high quality.

Croco – Wild! A surface that could make the viewer think of the skin of a crocodile. Naturally wild and fascinating beautiful - simply different.

**FRESCOLORI Croco**

Material: 1 CM7 layer

 1 CM1 layer

Consumption: CM7 about 1.2 kg/m² each layer

 CM1 about 0.4 kg/m² each layer

Colour : freely selectable

Application: Indoor

Surfaces are prepared and primed.

* Application of the first layer of the Caramor limestone-marble plaster, in grain thickness 7
* Immediate vertical or horizontal ribbing of the surface with thick edges
* Respect the waiting times with a rest period until the next day
* Application of the second layer of the Caramor limestone-marble plaster, in grain thickness 1, in the rib direction
* Observe the quite short waiting time (touch dry)
* Polish the surface with the trowel in the ribbing direction and against it