**FRESCOLORI Matt**

Delivery and servicing surfaces exclusively by trained FRESCOLORI processing specialists, with a long-term guarantee of high quality.

A lightweight, delicate surface with a fine natural radiance - a valued companion of timeless elegance.

**FRESCOLORI Matt**

Material: 2 CM3 layers

Consumption: CM3 about 1.0 kg/m² each layer

Colour : freely selectable

Application: Indoor

Surfaces are prepared and primed.

* Application of the first layer of the Caramor limestone-marble plaster, in grain thickness 3
* Observe the waiting times, with a rest period until the first layer is dry.
* Application of the second layer of the Caramor limestone-marble plaster, in grain thickness 3
* Humidify the surface with a long bristle brush/spray bottle with water, and prevent any running of the water on the surface
* Instant smooth the surface with a trowel, by applying a uniform pressure
* Smoothing the surface
* Observe the uniform distribution of the effluent limestone milk
* Observe the quite short waiting time (touch dry)
* Humidify the surface with a long bristle brush/spray bottle with water
* Instant smooth the surface with a trowel, by applying a uniform pressure