**FRESCOLORI Structure**

Delivery and servicing surfaces exclusively by trained FRESCOLORI processing specialists, with a long-term guarantee of high quality.

A wall design with a fine, light structure - smooth and humble. The surface is possible with light to strong smoothing while maintaining the light structure. A puristic charm, with a mineral appeal.

**FRESCOLORI Structure**

Material: 1 CM7 layer

Consumption: CM7 about 1.2 kg/m² each layer

Colour : freely selectable

Application: Indoor

Surfaces are prepared and primed.

* Apply the Caramor limestone-marble plaster in grain thickness 7
* Observe the quite short waiting time (touch dry)
* Humidify the surface with a long bristle brush/spray bottle with water, and prevent any running of the water on the surface
* Instant smooth the surface with a trowel, by applying a uniform pressure
* Observe the uniform distribution of the effluent limestone milk
* Design freedom: light or strong smoothing of the surface